# Om Metal Cast

Om Metal Cast has a wide range of products that meet the requirements of different kinds of automation used in different industries. Beginning as low as 1 kg, Om Metal Cast offers parts upto 500 kgs in weight and in a choice of several grades of Grey Iron Casting.

PREV NEXT
SINCE 2009

### AABOUT OUR COMPANY

##### WEL COME TO Om

Founded in 2009 under brand name of Om Metal Cast, we are engaged in to various manufacturing activities and had started primarily with focus on Exports markets. The founder duo, Mr. Milan Patel and Mr. Patel prior to 2006 were already engaged into Manufacturing and Export activities, heading a propitorship company engaged into Exports of High speed diesel engines, Fabricated mills, Merchant trading activities for supplies of Industrial consumables and turnkey projects.

#### 229

PRODUCTS

#### 169

TEAM

#### 203

FINISH PROJECT

#### 178

HAPPY CLIENTS

### CCASTING PROCESS

# 01 MOULDING

We have very good expertise in the following casting processes. We perform inspection process for moulds before pouring.We have several types of moulding like Greensand process, Molasses process,No bake process.

# 02 POURING & CASTING

We have two 21" Cupola furnace for the pouring, we use high grade pig Iron with required silicon content, while the melting the metal we perform carbon,silicon & manganese testing in ferro lab to ensure the raw material is PERFECT.

# 03 Shot blasting, Grinding and Fettling

The castings, after they are given sufficient time for cooling, undergo shot blasting process. Then they are brought to the Grinding and Fettling shop to remove any rough edges and other such casting defects.

# 04 Machining & Finishing

After Pouring once casting becomes at normal temperature to the atmosphere, we send casting for Shot blasting, Machining Grinding and Fettling to clean the casting After Finishing the casting we perform shot blasting process again to remove the machining and grinding scratches. Than we apply of coat of primer as per the customer's requirement.

# 05 Quality Control

We have been issued ISO 9001:2008 certification by TUV SUD Management Service GmbH and accordingly a stringent quality control program is followed which is implemented in the many phases.

# 06 PACKAGING & DISPETCH

After Pouring once casting becomes at normal temperature to the atmosphere, we send casting for Shot blasting, Machining Grinding and Fettling to clean the casting After Finishing the casting we perform shot blasting process again to remove the machining and grinding scratches. Than we apply of coat of primer as per the customer's requirement.

### QQUALITY

QUALITY POLICY

IPSUM 1992

CASTING IN PROCESS

IPSUM 1992

MACHINEING IN PROCESS

IPSUM 1992

PACKAGING IN PROCESS

IPSUM 1992

WE ARE HIRING TALENT, POST YOUR RESUME

POST