PROCESS
01

#### MOULDING

2 medium frequency furnaces with three crucibles of350 Kgs, 750 Kgs& 1000 Kgs, hence having the capacity of producing single piece casting of weight upto 1500 Kgs.CO2 process, No-Bake continuous mixer, Jolt-squeeze machine

02

#### POURING & CASTING

Bottom pouring ladle of capacity lip pouring ladle of capacity Tea-pot ladle of capacity.

03

#### Shot blasting, Grinding & Fettling

Knock-out using vibratory table, with Reclamation system and sand cooler system. 4-5 Swing Grinder 3-4 hand grinder pneumatic and electric table type SB machine Hanger type SB machine shot blasting room.

04

#### Machining & Finishing

Oil fired HT furnace of 8 Ton capacity; Electric HT Furnace fully automatic temperature controlled of 3 Ton Capacity: Rapid Water quenching arrangement; Water tank capacity of 85 KL.Conventional Lather machine, profile cutter Driling machine.

05

#### Quality Control

Chemical – Schimadzu make spectrometer with metal polishing facitlities; C-Si analyzer | Physical – Universal Testing machine, Rockwell Hardness Tester (FASNE Make), Brinell Hardness Tester (FIE Make), Metallurgical Microscope| NDT – Ultrasonic Testing Facility, Visual Inspection Area, Liquid Dye Penetration Test | Sand Testing – Universal Sand testing machinie, Sieve Shaker, Clay content tester, Moisture content tester, Muffle Furnace.

06

#### PACKAGING & DISPETCH

Login through the customer ID and Pwd provided and track the status of your order through the login section.

### PROCESS

It is a long established fact that a reader will be distracted by the readable content of a page when looking at its layout. The point of using Lorem Ipsum is that it has a more-or-less normal distribution of letters, as opposed to using 'Content here, content here', making it look like , sometimes on purpose (injected humour and the like).

READ MORE

### PROCESS

- 01 MOULDING
- 02 POURING & CASTING
- 03 Shot blasting, Grinding & Fettling
- 04 Machining & Finishing
- 05 Quality Control
- 06 PACKAGING & DISPETCH

### INSTAGRAM FEED