# TECHNICAL
DETAILS

###### POLE DIMENSIONS
150 mmx150mm, Length 4 feet to 12 feet groove width 60mm and depth 40mm.

###### POLE WEIGHT
14 kg/Rft (approx)

###### POLE REINFORCEMENT
3 mm dia.high tensile carbonized steel wire 7 nos.

###### PANEL DIMENSIONS
1 foot wide, 50 mm (2 inch thick)

###### PANEL WEIGHT
7'.0".X1'.0" Size 77 kg.( APPROX)

###### PANEL REINFORCEMENT
3 mm dia. high tensile carbonized steel wire 4 nos.

###### GRADE OF CONCRETE
M-25 Design max.

# TRADITIONAL vs. PRESTRESS PRECAST: WHAT’S THE BETTER CHOICE?

Sl.No. | Parameter | Traditional Boundary Wall | Prestress Precast Boundary Wall (PSPC BW) | Advantage PSPC BW
--- | --- | --- | --- | ---
1 | Erection time | A 100 meter wall takes a minimum of a week to construct and another week for curing | Same wall can be erected on site in just 2 days | Drastically reduces working time
2 | Longevity | Endurance of this wall depends on the quality of plaster used | PSPC panels are made of void-less dense high grade concrete | More durable
3 | Failure | In case of cover turning failure, a large section of the wall may be damaged and require almost new construction | In case of failure, only few columns may get damaged and require replacement; most panels can be reused with minor repairs | Almost zero repair costs and immediate correction
4 | Security | Its 150 mm thick brick masonry can be easily broken by ordinary hand tools | The panels are reinforced with high tensile wire - that can only be cut mechanically - at every 75 mm distance | Provides greater safety
5 | Climate impact | Plaster surface absorbs moisture, cracks, and peels off often | Hardly any moisture absorption as panel surfaces are made of dense concrete | Nearly nil maintenance cost
6 | Painting | Is essential as the plastered surface is not weatherproof | Optional, for aesthetic reasons | Cost savings
7 | Cleaning | Plaster attracts dust, fungus, algae, plants etc. and requires cleaning & painting at regular intervals | Merely washing can renew its looks | No extra effort and expense
8 | Reuse | Not possible as it is a permanent construction | 100% panels and 60% columns can be reused at another site | Slashes reinvestment costs
9 | Weight | Approximately 600 kg/RMT | Approximately 205 kg/RMT | Requires much smaller foundations