INFRASTRUCTURE

With the latest manufacturing unit located in Rajkot, Gujarat (INDIA), Om Metal Cast is one of the largest in the foundry industry. OM Metal Cast has a specific, yet continuous production process that caters to every function needed to produce a technologically superior casting component. Complete with melting, molding and core shops to development and quality control, OM Metal Cast takes every step necessary to creating the right component for every client in the shortest span of time.

##### Advanced Infrastructure

Factory is spread across total area of 5000 Sqmt in Village: Jhiyana- , 360023 Dist. Rajkot and has well infrastructure providing with ideal and healthy working environment. Corporate office is located in Rajkot City. Dedicated pattern storage area where all patterns are stored safely and with very easy traceability system (Computerised). Also, have in-house pattern workshop area where repair / modification of pattern work can be done. 2 medium frequency furnaces with three crucibles of350 Kgs, 750 Kgs& 1000 Kgs, hence having the capacity of producing single piece casting of weight upto 1500 Kgs.

##### HIGH QUALITY EQUIPMENT

CO2 process, No-Bake continuous mixer, Jolt-squeeze machine. Bottom pouring ladle of capacity ; lip pouring ladle of capacity ; Tea-pot ladle of capacity.Knock-out using vibratory table, with Reclamation system and sand cooler system. 4-5 Swing Grinder ; 3-4 hand grinder pneumatic and electric; table type SB machine; Hanger type SB machine; shot blasting room. Oil fired HT furnace of 8 Ton capacity; Electric HT Furnace fully automatic temperature controlled of 3 Ton Capacity: Rapid Water quenching arrangement; Water tank capacity of 85 KL Conventional Lather machine, profile cutter ;Driling machine. Chemical – Schimadzu make spectrometer with metal polishing facitlities; C-Si analyzer | Physical – Universal Testing machine, Rockwell Hardness Tester (FASNE Make), Brinell Hardness Tester (FIE Make), Metallurgical Microscope| NDT – Ultrasonic Testing Facility, Visual Inspection Area, Liquid Dye Penetration Test | Sand Testing – Universal Sand testing machinie, Sieve Shaker, Clay content tester, Moisture content tester, Muffle Furnace.

### OOUR SKILLS

Casting Stator case of MotorBody frame size 80 frame to 132 frame. Motor Body covers 80 frame to 225 frame size Submercible Pump Parts & other Pump parts like, Adaptop, Impellers, Casings, housings..